Dependencies for Project 'secure_bootloader_ble_s132_pca10040', Target 'nrf52832_xxaa_s132': (DO NOT MODIFY !)
CompilerVersion: 5060750::V5.06 update 6 (build 750)::.\ARMCC
F (.\main.c)(0x625D2912)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\main.o --omf_browse .\_build\main.crf --depend .\_build\main.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\boards\boards.h)(0x5F17D6B2)
I (..\..\..\..\..\modules\nrfx\hal\nrf_gpio.h)(0x607A6190)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\boards\pca10040.h)(0x6010E6E3)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_app_start.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_dfu_timers.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_ctrl.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_ctrl_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_backend_interface.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_default_backends.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\delay\nrf_delay.h)(0x5EE46ACE)
F (..\config\sdk_config.h)(0x626B4F25)()
F (.\dfu_public_key.c)(0x625D2912)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\dfu_public_key.o --omf_browse .\_build\dfu_public_key.crf --depend .\_build\dfu_public_key.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
F (..\..\..\..\..\components\boards\boards.c)(0x5FC21BCA)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\boards.o --omf_browse .\_build\boards.crf --depend .\_build\boards.d)
I (..\..\..\..\..\components\boards\boards.h)(0x5F17D6B2)
I (..\..\..\..\..\modules\nrfx\hal\nrf_gpio.h)(0x607A6190)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\boards\pca10040.h)(0x6010E6E3)
F (..\..\..\..\..\components\ble\common\ble_srv_common.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\ble_srv_common.o --omf_browse .\_build\ble_srv_common.crf --depend .\_build\ble_srv_common.d)
I (..\..\..\..\..\components\ble\common\ble_srv_common.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_l2cap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gatt.h)(0x60A8BEFE)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gattc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gatts.h)(0x5D5D198A)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_bootloader.o --omf_browse .\_build\nrf_bootloader.crf --depend .\_build\nrf_bootloader.d)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\boards\boards.h)(0x5F17D6B2)
I (..\..\..\..\..\modules\nrfx\hal\nrf_gpio.h)(0x607A6190)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\boards\pca10040.h)(0x6010E6E3)
I (..\..\..\..\..\modules\nrfx\hal\nrf_power.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\delay\nrf_delay.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_ctrl.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_ctrl_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_backend_interface.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_wdt.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_app_start.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_fw_activation.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_dfu_timers.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\scheduler\app_scheduler.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_validation.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\dfu-cc.pb.h)(0x5EE46ACD)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.h)(0x5EE46ACD)
F (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_app_start.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_bootloader_app_start.o --omf_browse .\_build\nrf_bootloader_app_start.crf --depend .\_build\nrf_bootloader_app_start.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_app_start.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_mbr.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log_ctrl.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_ctrl_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_backend_interface.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_app_start_final.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_bootloader_app_start_final.o --omf_browse .\_build\nrf_bootloader_app_start_final.crf --depend .\_build\nrf_bootloader_app_start_final.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_app_start.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_dfu_timers.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_bootloader_dfu_timers.o --omf_browse .\_build\nrf_bootloader_dfu_timers.crf --depend .\_build\nrf_bootloader_dfu_timers.d)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_dfu_timers.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\hal\nrf_clock.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\hal\nrf_rtc.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\delay\nrf_delay.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_fw_activation.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_bootloader_fw_activation.o --omf_browse .\_build\nrf_bootloader_fw_activation.crf --depend .\_build\nrf_bootloader_fw_activation.d)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_fw_activation.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_mbr.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crc32\crc32.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_ctrl.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_ctrl_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_backend_interface.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_wdt.h)(0x5EE46ACD)
F (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_bootloader_info.o --omf_browse .\_build\nrf_bootloader_info.crf --depend .\_build\nrf_bootloader_info.d)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\modules\nrfx\hal\nrf_nvmc.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
F (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_wdt.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_bootloader_wdt.o --omf_browse .\_build\nrf_bootloader_wdt.crf --depend .\_build\nrf_bootloader_wdt.d)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_wdt.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\modules\nrfx\hal\nrf_wdt.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_dfu_timers.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log_ctrl.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_ctrl_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\log\nrf_log_backend_interface.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_crypto_ecc.o --omf_browse .\_build\nrf_crypto_ecc.crf --depend .\_build\nrf_crypto_ecc.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_crypto_ecdsa.o --omf_browse .\_build\nrf_crypto_ecdsa.crf --depend .\_build\nrf_crypto_ecdsa.d)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
F (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_crypto_hash.o --omf_browse .\_build\nrf_crypto_hash.crf --depend .\_build\nrf_crypto_hash.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_sw\nrf_sw_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\sha256\sha256.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_shared.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\nrf_crypto_init.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_crypto_init.o --omf_browse .\_build\nrf_crypto_init.crf --depend .\_build\nrf_crypto_init.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_init.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\nrf_crypto_shared.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_crypto_shared.o --omf_browse .\_build\nrf_crypto_shared.crf --depend .\_build\nrf_crypto_shared.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
F (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_chacha_poly_aead.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\oberon_backend_chacha_poly_aead.o --omf_browse .\_build\oberon_backend_chacha_poly_aead.crf --depend .\_build\oberon_backend_chacha_poly_aead.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_chacha_poly_aead.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\oberon_backend_ecc.o --omf_browse .\_build\oberon_backend_ecc.crf --depend .\_build\oberon_backend_ecc.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
F (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdh.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\oberon_backend_ecdh.o --omf_browse .\_build\oberon_backend_ecdh.crf --depend .\_build\oberon_backend_ecdh.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
F (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdsa.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\oberon_backend_ecdsa.o --omf_browse .\_build\oberon_backend_ecdsa.crf --depend .\_build\oberon_backend_ecdsa.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
F (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_eddsa.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\oberon_backend_eddsa.o --omf_browse .\_build\oberon_backend_eddsa.crf --depend .\_build\oberon_backend_eddsa.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
F (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hash.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\oberon_backend_hash.o --omf_browse .\_build\oberon_backend_hash.crf --depend .\_build\oberon_backend_hash.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hmac.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\oberon_backend_hmac.o --omf_browse .\_build\oberon_backend_hmac.crf --depend .\_build\oberon_backend_hmac.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\crypto\backend\nrf_sw\nrf_sw_backend_hash.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_sw_backend_hash.o --omf_browse .\_build\nrf_sw_backend_hash.crf --depend .\_build\nrf_sw_backend_hash.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_sw\nrf_sw_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\sha256\sha256.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\micro_ecc_backend_ecc.o --omf_browse .\_build\micro_ecc_backend_ecc.crf --depend .\_build\micro_ecc_backend_ecc.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng_mbedtls.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_shared.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdh.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\micro_ecc_backend_ecdh.o --omf_browse .\_build\micro_ecc_backend_ecdh.crf --depend .\_build\micro_ecc_backend_ecdh.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_shared.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdsa.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\micro_ecc_backend_ecdsa.o --omf_browse .\_build\micro_ecc_backend_ecdsa.crf --depend .\_build\micro_ecc_backend_ecdsa.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_shared.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\dfu-cc.pb.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\dfu-cc.pb.o --omf_browse .\_build\dfu-cc.pb.crf --depend .\_build\dfu-cc.pb.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\dfu-cc.pb.h)(0x5EE46ACD)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu.o --omf_browse .\_build\nrf_dfu.crf --depend .\_build\nrf_dfu.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_transport.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\ble_dfu\nrf_dfu_ble.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_ble.o --omf_browse .\_build\nrf_dfu_ble.crf --depend .\_build\nrf_dfu_ble.d)
I (..\..\..\..\..\components\libraries\bootloader\ble_dfu\nrf_dfu_ble.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gatts.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gatt.h)(0x60A8BEFE)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_l2cap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gattc.h)(0x5D5D198A)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_transport.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_mbr.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\ble\common\ble_srv_common.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh_ble.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\balloc\nrf_balloc.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\delay\nrf_delay.h)(0x5EE46ACE)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_flash.o --omf_browse .\_build\nrf_dfu_flash.crf --depend .\_build\nrf_dfu_flash.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage_sd.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage_nvmc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_handling_error.o --omf_browse .\_build\nrf_dfu_handling_error.crf --depend .\_build\nrf_dfu_handling_error.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_mbr.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_mbr.o --omf_browse .\_build\nrf_dfu_mbr.crf --depend .\_build\nrf_dfu_mbr.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_mbr.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_req_handler.o --omf_browse .\_build\nrf_dfu_req_handler.crf --depend .\_build\nrf_dfu_req_handler.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (..\..\..\..\..\external\nano-pb\pb_common.h)(0x5EE43151)
I (..\..\..\..\..\external\nano-pb\pb_decode.h)(0x5EE43151)
I (..\..\..\..\..\components\libraries\bootloader\dfu\dfu-cc.pb.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\crc32\crc32.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\scheduler\app_scheduler.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_init.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_sw\nrf_sw_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\sha256\sha256.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng_mbedtls.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_chacha_poly_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cifra\cifra_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_chacha_poly_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hkdf.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_validation.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_settings.o --omf_browse .\_build\nrf_dfu_settings.crf --depend .\_build\nrf_dfu_settings.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\crc32\crc32.h)(0x5EE46ACE)
I (..\..\..\..\..\modules\nrfx\hal\nrf_nvmc.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings_svci.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_settings_svci.o --omf_browse .\_build\nrf_dfu_settings_svci.crf --depend .\_build\nrf_dfu_settings_svci.d)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\modules\nrfx\hal\nrf_nvmc.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\crc32\crc32.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_transport.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_transport.o --omf_browse .\_build\nrf_dfu_transport.crf --depend .\_build\nrf_dfu_transport.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_transport.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_utils.o --omf_browse .\_build\nrf_dfu_utils.crf --depend .\_build\nrf_dfu_utils.d)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crc32\crc32.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_validation.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\dfu-cc.pb.h)(0x5EE46ACD)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_validation.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_validation.o --omf_browse .\_build\nrf_dfu_validation.crf --depend .\_build\nrf_dfu_validation.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (..\..\..\..\..\external\nano-pb\pb_common.h)(0x5EE43151)
I (..\..\..\..\..\external\nano-pb\pb_decode.h)(0x5EE43151)
I (..\..\..\..\..\components\libraries\bootloader\dfu\dfu-cc.pb.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\crc32\crc32.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_init.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_sw\nrf_sw_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\sha256\sha256.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng_mbedtls.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_chacha_poly_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cifra\cifra_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_chacha_poly_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hkdf.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_validation.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_ver_validation.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\strerror\nrf_strerror.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_ctrl.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_ctrl_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_backend_interface.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_ver_validation.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_ver_validation.o --omf_browse .\_build\nrf_dfu_ver_validation.crf --depend .\_build\nrf_dfu_ver_validation.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_utils.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\nrf_bootloader_info.h)(0x5EE46ACD)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_init.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_mem.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_alloca.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\alloca.h)(0x5E53505A)
I (..\arm5_no_packs\nrf_crypto_allocator.h)(0x625D2912)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_error.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecc_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\external\micro-ecc\micro-ecc\uECC.h)(0x59487FE1)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hash_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_sw\nrf_sw_backend_hash.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\sha256\sha256.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_ecdh_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310_bl\cc310_bl_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\micro_ecc\micro_ecc_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_ecdh.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_rng_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\nrf_hw\nrf_hw_backend_rng_mbedtls.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\optiga\optiga_backend_rng.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aes_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_aes.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_aead_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_chacha_poly_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cifra\cifra_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_aes_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_chacha_poly_aead.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hmac_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\mbedtls\mbedtls_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_hmac.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_hkdf.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa_shared.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\nrf_crypto_eddsa_backend.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\cc310\cc310_backend_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\crypto\backend\oberon\oberon_backend_eddsa.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\dfu-cc.pb.h)(0x5EE46ACD)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_ver_validation.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_handling_error.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_req_handler.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\modules\nrfx\hal\nrf_nvmc.c)(0x5EE46AD4)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_nvmc.o --omf_browse .\_build\nrf_nvmc.crf --depend .\_build\nrf_nvmc.d)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\hal\nrf_nvmc.h)(0x5EE46AD4)
F (..\..\..\..\..\modules\nrfx\soc\nrfx_atomic.c)(0x5EE46AD4)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrfx_atomic.o --omf_browse .\_build\nrfx_atomic.crf --depend .\_build\nrfx_atomic.d)
I (..\..\..\..\..\modules\nrfx\soc\nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc\nrfx_atomic_internal.h)(0x5EE46AD4)
F (..\..\..\..\..\components\libraries\util\app_error_weak.c)(0x60AF17BE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\app_error_weak.o --omf_browse .\_build\app_error_weak.crf --depend .\_build\app_error_weak.d)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_ctrl.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_ctrl_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_backend_interface.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\strerror\nrf_strerror.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
F (..\..\..\..\..\components\libraries\scheduler\app_scheduler.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\app_scheduler.o --omf_browse .\_build\app_scheduler.crf --depend .\_build\app_scheduler.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\scheduler\app_scheduler.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
F (..\..\..\..\..\components\libraries\util\app_util_platform.c)(0x5EE46ACF)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\app_util_platform.o --omf_browse .\_build\app_util_platform.crf --depend .\_build\app_util_platform.d)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\crc32\crc32.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\crc32.o --omf_browse .\_build\crc32.crf --depend .\_build\crc32.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\crc32\crc32.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x5E53505C)
F (..\..\..\..\..\components\libraries\mem_manager\mem_manager.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\mem_manager.o --omf_browse .\_build\mem_manager.crf --depend .\_build\mem_manager.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\mem_manager\mem_manager.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\util\nrf_assert.c)(0x5EE46ACF)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_assert.o --omf_browse .\_build\nrf_assert.crf --depend .\_build\nrf_assert.d)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\atomic_fifo\nrf_atfifo.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_atfifo.o --omf_browse .\_build\nrf_atfifo.crf --depend .\_build\nrf_atfifo.d)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\atomic_fifo\nrf_atfifo.h)(0x5EE46ACD)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\atomic_fifo\nrf_atfifo_internal.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\atomic\nrf_atomic.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_atomic.o --omf_browse .\_build\nrf_atomic.crf --depend .\_build\nrf_atomic.d)
I (..\..\..\..\..\components\libraries\atomic\nrf_atomic.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\atomic\nrf_atomic_internal.h)(0x5EE46ACD)
F (..\..\..\..\..\components\libraries\balloc\nrf_balloc.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_balloc.o --omf_browse .\_build\nrf_balloc.crf --depend .\_build\nrf_balloc.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\balloc\nrf_balloc.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
F (..\..\..\..\..\external\fprintf\nrf_fprintf.c)(0x5EE46AD4)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_fprintf.o --omf_browse .\_build\nrf_fprintf.crf --depend .\_build\nrf_fprintf.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdarg.h)(0x5E53505C)
I (..\..\..\..\..\external\fprintf\nrf_fprintf_format.h)(0x5EE43150)
I (..\..\..\..\..\external\fprintf\nrf_fprintf.h)(0x5EE46AD4)
F (..\..\..\..\..\external\fprintf\nrf_fprintf_format.c)(0x5EE43150)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_fprintf_format.o --omf_browse .\_build\nrf_fprintf_format.crf --depend .\_build\nrf_fprintf_format.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdarg.h)(0x5E53505C)
I (..\..\..\..\..\external\fprintf\nrf_fprintf.h)(0x5EE46AD4)
I (..\..\..\..\..\external\fprintf\nrf_fprintf_format.h)(0x5EE43150)
F (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_fstorage.o --omf_browse .\_build\nrf_fstorage.crf --depend .\_build\nrf_fstorage.d)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage_nvmc.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_fstorage_nvmc.o --omf_browse .\_build\nrf_fstorage_nvmc.crf --depend .\_build\nrf_fstorage_nvmc.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage_nvmc.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\modules\nrfx\hal\nrf_nvmc.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\atomic\nrf_atomic.h)(0x5EE46ACD)
F (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage_sd.c)(0x62973A6C)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_fstorage_sd.o --omf_browse .\_build\nrf_fstorage_sd.crf --depend .\_build\nrf_fstorage_sd.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage_sd.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\fstorage\nrf_fstorage.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh_soc.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\atomic\nrf_atomic.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\atomic_fifo\nrf_atfifo.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\memobj\nrf_memobj.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_memobj.o --omf_browse .\_build\nrf_memobj.crf --depend .\_build\nrf_memobj.d)
I (..\..\..\..\..\components\libraries\memobj\nrf_memobj.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\balloc\nrf_balloc.h)(0x5EE46ACD)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\atomic\nrf_atomic.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\queue\nrf_queue.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_queue.o --omf_browse .\_build\nrf_queue.crf --depend .\_build\nrf_queue.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\ringbuf\nrf_ringbuf.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_ringbuf.o --omf_browse .\_build\nrf_ringbuf.crf --depend .\_build\nrf_ringbuf.d)
I (..\..\..\..\..\components\libraries\ringbuf\nrf_ringbuf.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\atomic\nrf_atomic.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_section_iter.o --omf_browse .\_build\nrf_section_iter.crf --depend .\_build\nrf_section_iter.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\strerror\nrf_strerror.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_strerror.o --omf_browse .\_build\nrf_strerror.crf --depend .\_build\nrf_strerror.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\strerror\nrf_strerror.h)(0x5EE46ACE)
F (..\..\..\..\..\components\libraries\sha256\sha256.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\sha256.o --omf_browse .\_build\sha256.crf --depend .\_build\sha256.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdlib.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\sha256\sha256.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\log\src\nrf_log_frontend.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_log_frontend.o --omf_browse .\_build\nrf_log_frontend.crf --depend .\_build\nrf_log_frontend.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
F (..\..\..\..\..\components\libraries\log\src\nrf_log_str_formatter.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_log_str_formatter.o --omf_browse .\_build\nrf_log_str_formatter.crf --depend .\_build\nrf_log_str_formatter.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
F (..\..\..\..\..\external\nrf_oberon\lib\cortex-m4\hard-float\short-wchar\oberon_3.0.5.lib)(0x5EE43174)()
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_svci.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_svci.o --omf_browse .\_build\nrf_dfu_svci.crf --depend .\_build\nrf_dfu_svci.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
F (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_svci_handler.c)(0x5EE46ACD)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_dfu_svci_handler.o --omf_browse .\_build\nrf_dfu_svci_handler.crf --depend .\_build\nrf_dfu_svci_handler.d)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\svc\nrf_svci_async_handler.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\svc\nrf_svc_function.h)(0x5EE46ACE)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\svc\nrf_svci.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\hal\nrf_nvmc.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\nrfx.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\nrfx_config.h)(0x60EFFB44)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_common.h)(0x5EE46AD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_peripherals.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52832_peripherals.h)(0x5E5F5130)
I (..\..\..\..\..\integration\nrfx\nrfx_glue.h)(0x5EE46AD4)
I (..\..\..\..\..\integration\nrfx\legacy/apply_old_config.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_irqs_nrf52832.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_coredep.h)(0x5EE46AD4)
I (..\..\..\..\..\modules\nrfx\soc/nrfx_atomic.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\util\sdk_resources.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sd_def.h)(0x5EE46ACF)
I (..\..\..\..\..\modules\nrfx\drivers/nrfx_errors.h)(0x5EE46AD4)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_types.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\bootloader\ble_dfu\nrf_dfu_ble_svci_bond_sharing.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\svc\nrf_svci_async_function.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_settings.h)(0x5EE46ACD)
I (..\..\..\..\..\components\libraries\bootloader\dfu\nrf_dfu_flash.h)(0x5EE46ACD)
F (..\..\..\..\..\components\libraries\svc\nrf_svc_handler.c)(0x5EE46ACE)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_svc_handler.o --omf_browse .\_build\nrf_svc_handler.crf --depend .\_build\nrf_svc_handler.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\svc\nrf_svc_function.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\svc\nrf_svci.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
F (..\..\..\..\..\components\softdevice\common\nrf_sdh.c)(0x5EE46ACF)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_sdh.o --omf_browse .\_build\nrf_sdh.crf --depend .\_build\nrf_sdh.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_sdm.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_nvic.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_util_platform.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\softdevice\common\nrf_sdh_ble.c)(0x5EE46ACF)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_sdh_ble.o --omf_browse .\_build\nrf_sdh_ble.crf --depend .\_build\nrf_sdh_ble.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh_ble.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\ble.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_err.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_hci.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_ranges.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_types.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_l2cap.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gatt.h)(0x60A8BEFE)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gattc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\ble_gatts.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\strerror\nrf_strerror.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\components\softdevice\common\nrf_sdh_soc.c)(0x5EE46ACF)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\nrf_sdh_soc.o --omf_browse .\_build\nrf_sdh_soc.crf --depend .\_build\nrf_sdh_soc.d)
I (..\..\..\..\..\components\libraries\util\sdk_common.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\config\sdk_config.h)(0x626B4F25)
I (..\..\..\..\..\components\libraries\util\nordic_common.h)(0x5F1F8589)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (..\..\..\..\..\components\libraries\util\sdk_os.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\sdk_errors.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\app_util.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf52\nrf_mbr.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_svc.h)(0x5D5D198A)
I (..\..\..\..\..\components\libraries\util\sdk_macros.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\nrf_assert.h)(0x5EE46ACF)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh_soc.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section.h)(0x5EE46ACE)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\s132\headers\nrf_error_soc.h)(0x5D5D198A)
I (..\..\..\..\..\components\softdevice\common\nrf_sdh.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\util\app_error.h)(0x5EE46ACF)
I (C:\Keil_v5\ARM\ARMCC\include\stdio.h)(0x5E53505C)
I (..\..\..\..\..\components\libraries\util\app_error_weak.h)(0x5EE46ACF)
I (..\..\..\..\..\components\libraries\log\nrf_log.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\src\nrf_log_internal.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_instance.h)(0x5EE46ACE)
I (..\..\..\..\..\components\libraries\log\nrf_log_types.h)(0x5EE46ACE)
F (..\..\..\..\..\external\micro-ecc\nrf52hf_keil\armgcc\micro_ecc_lib_nrf52.lib)(0x5C11C001)()
F (..\..\..\..\..\external\nano-pb\pb_common.c)(0x5EE43151)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\pb_common.o --omf_browse .\_build\pb_common.crf --depend .\_build\pb_common.d)
I (..\..\..\..\..\external\nano-pb\pb_common.h)(0x5EE43151)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
F (..\..\..\..\..\external\nano-pb\pb_decode.c)(0x5EE43151)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\pb_decode.o --omf_browse .\_build\pb_decode.crf --depend .\_build\pb_decode.d)
I (..\..\..\..\..\external\nano-pb\pb.h)(0x5EE43151)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stddef.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\string.h)(0x5E53505C)
I (..\..\..\..\..\external\nano-pb\pb_decode.h)(0x5EE43151)
I (..\..\..\..\..\external\nano-pb\pb_common.h)(0x5EE43151)
F (RTE\Device\nRF52832_xxAA\arm_startup_nrf52.s)(0x625D2912)(--cpu Cortex-M4.fp.sp -g --apcs=interwork --pd "__MICROLIB SETA 1" -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config  --cpreproc_opts=-DBLE_STACK_SUPPORT_REQD,-DBOARD_PCA10040,-DCONFIG_GPIO_AS_PINRESET,-DFLOAT_ABI_HARD,-DNRF52,-DNRF52832_XXAA,-DNRF52_PAN_74,-DNRF_DFU_SETTINGS_VERSION=2,-DNRF_DFU_SVCI_ENABLED,-DNRF_SD_BLE_API_VERSION=7,-DS132,-DSOFTDEVICE_PRESENT,-DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION,-D__HEAP_SIZE=0,-DuECC_ENABLE_VLI_API=0,-DuECC_OPTIMIZATION_LEVEL=3,-DuECC_SQUARE_FUNC=0,-DuECC_SUPPORT_COMPRESSED_POINT=0,-DuECC_VLI_NATIVE_LITTLE_ENDIAN=1

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

--pd "__UVISION_VERSION SETA 530" --pd "_RTE_ SETA 1" --pd "NRF52832_XXAA SETA 1" --pd "_RTE_ SETA 1" --pd "BLE_STACK_SUPPORT_REQD SETA 1" --pd "BOARD_PCA10040 SETA 1" --pd "CONFIG_GPIO_AS_PINRESET SETA 1" --pd "FLOAT_ABI_HARD SETA 1" --pd "NRF52 SETA 1" --pd "NRF52832_XXAA SETA 1" --pd "NRF52_PAN_74 SETA 1" --pd "NRF_DFU_SETTINGS_VERSION SETA 2" --pd "NRF_DFU_SVCI_ENABLED SETA 1" --pd "NRF_SD_BLE_API_VERSION SETA 7" --pd "S132 SETA 1" --pd "SOFTDEVICE_PRESENT SETA 1" --pd "SVC_INTERFACE_CALL_AS_NORMAL_FUNCTION SETA 1" --pd "__HEAP_SIZE SETA 0" --pd "uECC_ENABLE_VLI_API SETA 0" --pd "uECC_OPTIMIZATION_LEVEL SETA 3" --pd "uECC_SQUARE_FUNC SETA 0" --pd "uECC_SUPPORT_COMPRESSED_POINT SETA 0" --pd "uECC_VLI_NATIVE_LITTLE_ENDIAN SETA 1"

--list .\_build\arm_startup_nrf52.lst --xref -o .\_build\arm_startup_nrf52.o --depend .\_build\arm_startup_nrf52.d)
F (RTE\Device\nRF52832_xxAA\system_nrf52.c)(0x625D2912)(--c99 -c --cpu Cortex-M4.fp.sp -D__MICROLIB -g -O3 --apcs=interwork --split_sections -I ..\..\config -I ..\..\..\..\..\components\ble\common -I ..\..\..\..\..\components\boards -I ..\..\..\..\..\components\libraries\atomic -I ..\..\..\..\..\components\libraries\atomic_fifo -I ..\..\..\..\..\components\libraries\balloc -I ..\..\..\..\..\components\libraries\bootloader -I ..\..\..\..\..\components\libraries\bootloader\ble_dfu -I ..\..\..\..\..\components\libraries\bootloader\dfu -I ..\..\..\..\..\components\libraries\crc32 -I ..\..\..\..\..\components\libraries\crypto -I ..\..\..\..\..\components\libraries\crypto\backend\cc310 -I ..\..\..\..\..\components\libraries\crypto\backend\cc310_bl -I ..\..\..\..\..\components\libraries\crypto\backend\cifra -I ..\..\..\..\..\components\libraries\crypto\backend\mbedtls -I ..\..\..\..\..\components\libraries\crypto\backend\micro_ecc -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_hw -I ..\..\..\..\..\components\libraries\crypto\backend\nrf_sw -I ..\..\..\..\..\components\libraries\crypto\backend\oberon -I ..\..\..\..\..\components\libraries\crypto\backend\optiga -I ..\..\..\..\..\components\libraries\delay -I ..\..\..\..\..\components\libraries\experimental_section_vars -I ..\..\..\..\..\components\libraries\fstorage -I ..\..\..\..\..\components\libraries\log -I ..\..\..\..\..\components\libraries\log\src -I ..\..\..\..\..\components\libraries\mem_manager -I ..\..\..\..\..\components\libraries\memobj -I ..\..\..\..\..\components\libraries\queue -I ..\..\..\..\..\components\libraries\ringbuf -I ..\..\..\..\..\components\libraries\scheduler -I ..\..\..\..\..\components\libraries\sha256 -I ..\..\..\..\..\components\libraries\stack_info -I ..\..\..\..\..\components\libraries\strerror -I ..\..\..\..\..\components\libraries\svc -I ..\..\..\..\..\components\libraries\util -I ..\..\..\..\..\components\softdevice\common -I ..\..\..\..\..\components\softdevice\s132\headers -I ..\..\..\..\..\components\softdevice\s132\headers\nrf52 -I ..\.. -I ..\..\..\..\..\external\fprintf -I ..\..\..\..\..\external\micro-ecc\micro-ecc -I ..\..\..\..\..\external\nano-pb -I ..\..\..\..\..\external\nrf_oberon -I ..\..\..\..\..\external\nrf_oberon\include -I ..\..\..\..\..\integration\nrfx -I ..\..\..\..\..\modules\nrfx -I ..\..\..\..\..\modules\nrfx\hal -I ..\config -I ..\arm5_no_packs --reduce_paths

-I.\RTE\_nrf52832_xxaa_s132

-IC:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include

-IC:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include

-D__UVISION_VERSION="530" -D_RTE_ -DNRF52832_XXAA -D_RTE_ -DBLE_STACK_SUPPORT_REQD -DBOARD_PCA10040 -DCONFIG_GPIO_AS_PINRESET -DFLOAT_ABI_HARD -DNRF52 -DNRF52832_XXAA -DNRF52_PAN_74 -DNRF_DFU_SETTINGS_VERSION="2" -DNRF_DFU_SVCI_ENABLED -DNRF_SD_BLE_API_VERSION="7" -DS132 -DSOFTDEVICE_PRESENT -DSVC_INTERFACE_CALL_AS_NORMAL_FUNCTION -D__HEAP_SIZE="0" -DuECC_ENABLE_VLI_API="0" -DuECC_OPTIMIZATION_LEVEL="3" -DuECC_SQUARE_FUNC="0" -DuECC_SUPPORT_COMPRESSED_POINT="0" -DuECC_VLI_NATIVE_LITTLE_ENDIAN="1"

-o .\_build\system_nrf52.o --omf_browse .\_build\system_nrf52.crf --depend .\_build\system_nrf52.d)
I (C:\Keil_v5\ARM\ARMCC\include\stdint.h)(0x5E53505C)
I (C:\Keil_v5\ARM\ARMCC\include\stdbool.h)(0x5E53505C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf.h)(0x5E5F512C)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52.h)(0x5E5F5134)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\core_cm4.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_version.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_compiler.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\cmsis_armcc.h)(0x5D2590B6)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\ARM\CMSIS\5.6.0\CMSIS\Core\Include\mpu_armv7.h)(0x5C8F4DD4)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\system_nrf52.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_bitfields.h)(0x5E5F5126)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_to_nrf52.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_name_change.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\compiler_abstraction.h)(0x5E5F512E)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf_erratas.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf51_erratas.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf52_erratas.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf53_erratas.h)(0x5E5F5132)
I (C:\Users\Administrator\AppData\Local\Arm\Packs\NordicSemiconductor\nRF_DeviceFamilyPack\8.32.1\Device\Include\nrf91_erratas.h)(0x5E5F5132)
