T2C4C 000:167.264   SEGGER J-Link V7.56a Log File
T2C4C 000:167.566   DLL Compiled: Oct 11 2021 16:27:21
T2C4C 000:167.582   Logging started @ 2022-07-26 01:59
T2C4C 000:167.595 - 167.602ms
T2C4C 000:167.621 JLINK_SetWarnOutHandler(...)
T2C4C 000:167.638 - 0.024ms
T2C4C 000:167.657 JLINK_OpenEx(...)
T2C4C 000:175.824   Firmware: J-Link V9 compiled May  7 2021 16:26:12
T2C4C 000:176.901   Firmware: J-Link V9 compiled May  7 2021 16:26:12
T2C4C 000:177.391   Decompressing FW timestamp took 417 us
T2C4C 000:188.602   Hardware: V9.40
T2C4C 000:188.649   S/N: 99452020
T2C4C 000:188.670   OEM: SEGGER
T2C4C 000:188.690   Feature(s): RDI, GDB, FlashDL, FlashBP, JFlash
T2C4C 000:196.454   TELNET listener socket opened on port 19021
T2C4C 000:196.835   WEBSRV WEBSRV_Init(): Starting webserver thread(s)
T2C4C 000:197.003   WEBSRV Failed to put socket into listener state (port 19080)
T2C4C 000:197.242   WEBSRV Webserver running on local port 19081
T2C4C 000:231.407 - 63.782ms returns "O.K."
T2C4C 000:231.559 JLINK_GetEmuCaps()
T2C4C 000:231.577 - 0.025ms returns 0xB9FF7BBF
T2C4C 000:231.634 JLINK_TIF_GetAvailable(...)
T2C4C 000:233.467 - 1.857ms
T2C4C 000:233.560 JLINK_SetErrorOutHandler(...)
T2C4C 000:233.577 - 0.024ms
T2C4C 000:233.627 JLINK_ExecCommand("ProjectFile = "D:\Git_Project\shoes\smart_shoes\nRF5_SDK_17.0.0_9d13099\examples\Shoes1.3\shoe_mcu\pca10040\s132\arm5_no_packs\JLinkSettings.ini"", ...). 
T2C4C 000:267.285   Ref file found at: C:\Keil_v5\ARM\Segger\JLinkDevices.ref
T2C4C 000:267.480   XML referenced by ref file: C:\Program Files\SEGGER\JLink\JLinkDevices.xml
T2C4C 000:268.706   C:\Program Files\SEGGER\JLink\JLinkDevices.xml evaluated successfully.
T2C4C 000:346.184 - 112.566ms returns 0x00
T2C4C 000:346.214 JLINK_ExecCommand("Device = nRF52832_xxAA", ...). 
T2C4C 000:346.446   Device "NRF52832_XXAA" selected.
T2C4C 000:346.649 - 0.432ms returns 0x00
T2C4C 000:346.663 JLINK_ExecCommand("DisableConnectionTimeout", ...). 
T2C4C 000:346.672 - 0.004ms returns 0x01
T2C4C 000:346.684 JLINK_GetHardwareVersion()
T2C4C 000:346.689 - 0.007ms returns 94000
T2C4C 000:346.697 JLINK_GetDLLVersion()
T2C4C 000:346.702 - 0.007ms returns 75601
T2C4C 000:346.708 JLINK_GetOEMString(...)
T2C4C 000:346.715 JLINK_GetFirmwareString(...)
T2C4C 000:346.720 - 0.007ms
T2C4C 000:346.729 JLINK_GetDLLVersion()
T2C4C 000:346.734 - 0.007ms returns 75601
T2C4C 000:346.741 JLINK_GetCompileDateTime()
T2C4C 000:346.746 - 0.007ms
T2C4C 000:346.755 JLINK_GetFirmwareString(...)
T2C4C 000:346.760 - 0.007ms
T2C4C 000:346.767 JLINK_GetHardwareVersion()
T2C4C 000:346.772 - 0.007ms returns 94000
T2C4C 000:346.780 JLINK_GetSN()
T2C4C 000:346.785 - 0.007ms returns 99452020
T2C4C 000:346.793 JLINK_GetOEMString(...)
T2C4C 000:346.802 JLINK_TIF_Select(JLINKARM_TIF_SWD)
T2C4C 000:349.441 - 2.645ms returns 0x00
T2C4C 000:349.473 JLINK_HasError()
T2C4C 000:349.485 JLINK_SetSpeed(5000)
T2C4C 000:355.659 - 6.182ms
T2C4C 000:355.968 JLINK_HasError()
T2C4C 000:355.979 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)
T2C4C 000:355.984 - 0.007ms returns JLINKARM_RESET_TYPE_NORMAL
T2C4C 000:355.991 JLINK_Reset()
T2C4C 000:361.085   InitTarget() start
T2C4C 000:361.096    J-Link Script File: Executing InitTarget()
T2C4C 000:365.255   InitTarget() end
T2C4C 000:366.280   Found SW-DP with ID 0x2BA01477
T2C4C 000:369.657   DPIDR: 0x2BA01477
T2C4C 000:369.674   Scanning AP map to find all available APs
T2C4C 000:371.155   AP[2]: Stopped AP scan as end of AP map has been reached
T2C4C 000:371.169   AP[0]: AHB-AP (IDR: 0x24770011)
T2C4C 000:371.176   AP[1]: JTAG-AP (IDR: 0x02880000)
T2C4C 000:371.184   Iterating through AP map to find AHB-AP to use
T2C4C 000:372.449   AP[0]: Core found
T2C4C 000:372.460   AP[0]: AHB-AP ROM base: 0xE00FF000
T2C4C 000:373.097   CPUID register: 0x410FC241. Implementer code: 0x41 (ARM)
T2C4C 000:373.108   Found Cortex-M4 r0p1, Little endian.
T2C4C 000:475.128   -- Max. mem block: 0x0000D538
T2C4C 000:479.760   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C4C 000:480.680   CPU_ReadMem(4 bytes @ 0xE0002000)
T2C4C 000:481.806   FPUnit: 6 code (BP) slots and 2 literal slots
T2C4C 000:481.855   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T2C4C 000:482.696   CPU_ReadMem(4 bytes @ 0xE0001000)
T2C4C 000:483.535   CPU_WriteMem(4 bytes @ 0xE0001000)
T2C4C 000:484.512   CPU_ReadMem(4 bytes @ 0xE000ED88)
T2C4C 000:485.284   CPU_WriteMem(4 bytes @ 0xE000ED88)
T2C4C 000:486.099   CPU_ReadMem(4 bytes @ 0xE000ED88)
T2C4C 000:487.216   CPU_WriteMem(4 bytes @ 0xE000ED88)
T2C4C 000:488.089   CoreSight components:
T2C4C 000:488.138   ROMTbl[0] @ E00FF000
T2C4C 000:488.173   CPU_ReadMem(64 bytes @ 0xE00FF000)
T2C4C 000:489.289   CPU_ReadMem(32 bytes @ 0xE000EFE0)
T2C4C 000:490.294   [0][0]: E000E000 CID B105E00D PID 000BB00C SCS-M7
T2C4C 000:490.342   CPU_ReadMem(32 bytes @ 0xE0001FE0)
T2C4C 000:491.369   [0][1]: E0001000 CID B105E00D PID 003BB002 DWT
T2C4C 000:491.416   CPU_ReadMem(32 bytes @ 0xE0002FE0)
T2C4C 000:492.353   [0][2]: E0002000 CID B105E00D PID 002BB003 FPB
T2C4C 000:492.400   CPU_ReadMem(32 bytes @ 0xE0000FE0)
T2C4C 000:493.398   [0][3]: E0000000 CID B105E00D PID 003BB001 ITM
T2C4C 000:493.445   CPU_ReadMem(32 bytes @ 0xE0040FE0)
T2C4C 000:494.421   [0][4]: E0040000 CID B105900D PID 000BB9A1 TPIU
T2C4C 000:494.469   CPU_ReadMem(32 bytes @ 0xE0041FE0)
T2C4C 000:495.448   [0][5]: E0041000 CID B105900D PID 000BB925 ETM
T2C4C 000:497.801   CPU is running
T2C4C 000:497.855   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T2C4C 000:498.730   CPU is running
T2C4C 000:498.778   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T2C4C 000:499.671   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T2C4C 000:501.175   Reset: Reset device via AIRCR.SYSRESETREQ.
T2C4C 000:501.231   CPU is running
T2C4C 000:501.268   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T2C4C 000:556.233   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C4C 000:557.122   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C4C 000:557.988   CPU is running
T2C4C 000:558.037   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T2C4C 000:558.938   CPU is running
T2C4C 000:558.987   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T2C4C 000:565.744   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C4C 000:570.172   CPU_WriteMem(4 bytes @ 0xE0002000)
T2C4C 000:571.076   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T2C4C 000:572.365   CPU_ReadMem(4 bytes @ 0xE0001000)
T2C4C 000:573.554 - 217.587ms
T2C4C 000:573.671 JLINK_GetId()
T2C4C 000:574.527 - 0.881ms returns 0x2BA01477
T2C4C 000:588.137 JLINK_GetFirmwareString(...)
T2C4C 000:588.188 - 0.062ms
T2C4C 000:955.719 JLINK_Close()
T2C4C 000:956.358   CPU_ReadMem(4 bytes @ 0xE0001000)
T2C4C 000:956.947   CPU_WriteMem(4 bytes @ 0xE0001004)
T2C4C 000:969.313 - 13.614ms
T2C4C 000:969.338   
T2C4C 000:969.344   Closed
