{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":32,"n_cols":11,"rows_kept":32,"cut":false,"hidden":false,"merged":[[0,0,0,8]]}
["R BOM-75PCS"]
["序号","名称","型号","封装","位号","用量","总用量","采购数量","单价","总金额","备注"]
[1,"贴片电容","0.1uF","0402C","C1, C7, C9, C14, C15, C17",6,{"$f":"F3*75","v":450},{"$f":"F3*80","v":480},null,10,"50V"]
[2,"贴片电容","10uF","0402C","C2",1,{"$f":"F4*75","v":75},{"$f":"F4*80","v":80},null,9,"10V"]
[3,"贴片电容","22uF","0805C","C3, C5, C16, C19",4,300,320,null,43,"25V"]
[4,"贴片电容","1uF","0402C","C4, C18",2,150,160,null,8,"25V"]
[5,"贴片电容","2.2uF","0402C","C6",1,75,80,null,14,"25V"]
[6,"贴片电容","12pF","0402C","C8, C10",2,150,160,null,4,"50V"]
[7,"贴片电容","100pF","0402C","C11",1,75,80,null,2,"50V"]
[8,"贴片电容","1.0pF","0402C","C13",1,75,80,null,2,"50V"]
[9,"贴片电容","10uF","0805C","C24",1,75,80,null,10,"25V"]
[10,"贴片二极管","SS14","SOD-323","D1, D3",2,150,160,0.3,{"$f":"H12*I12","v":48}]
[11,"贴片LED灯","红光LED灯","0402LED","D2",1,75,80,null,8]
[12,"贴片连接器","SH连接器，5P，1.0mm间距，卧式","SH1.0-5AW","J2",1,75,80,0.25,{"$f":"H14*I14","v":20},"编带"]
[13,"贴片电感","3.3nH","0402L","L3",1,75,80,null,6]
[14,"贴片三极管","AO3401","SOT-23-3","Q1",1,75,80,0.7,{"$f":"H16*I16","v":56}]
[15,"贴片三极管","AO3400","SOT-23","Q2",1,75,80,0.75,{"$f":"H17*I17","v":60}]
[16,"贴片电阻","3K/1%","0603RM","R1",1,75,80,null,2]
[17,"贴片电阻","200K/1%","0402R","R2",1,75,80,null,2]
[18,"贴片电阻","300K/1%","0402R","R3",1,75,80,null,2]
[19,"贴片电阻","100K","0402R","R4, R5",2,150,160,null,2]
[20,"贴片电阻","0R","0402R","R6, R9",2,150,160,null,2]
[21,"贴片电阻","1K","0402R","R7, R10, R11, R12",4,300,320,null,3]
[22,"贴片电阻","4.7K","0402R","R8",1,75,80,null,2]
[23,"贴片电阻","10R","0603R","R13",1,75,80,null,2]
[24,"贴片电阻","10K","0402R","R14",1,75,80,null,2]
[25,"芯片","TP4056X","SOP-8P","U1",1,75,75,1.2,{"$f":"H27*I27","v":90}]
[26,"芯片","NRF52832-QFAA-R","QFN48P-6X6","U3",1,75,75,45,{"$f":"H28*I28","v":3375}]
[27,"芯片","XC6206P302MR","SOT-23","U4",1,75,80,0.6,48,"TOREX/特瑞仕"]
[28,"芯片","MT9700","SOT-23-5","U7",1,75,80,0.65,52]
[29,"晶振","32MHz/12pF/10PPM","XTAL-SMD-2016","Y1",1,75,80,0.85,68]
[{"$nulls":9},{"$f":"SUM(J3:J31)","v":3952}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}