{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":11,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,7]]}
["前脚 BOM-150PCS"]
["序号","名称","型号","封装","位号","用量","总用量","采购数量","单价","总金额","备注"]
[1,"贴片电容","1uF","0402C","C1, C2, C3, C4",4,{"$f":"F3*150","v":600},630,null,20,"25V"]
[2,"贴片电容","10uF","0603C","C5",1,{"$f":"F4*150","v":150},170,null,20,"26V"]
[3,"芯片","LSM6DS3TR-C","LGA-14_2.5*3-e0.5","U1",1,150,150,9.6,{"$f":"H5*I5","v":1440}]
[4,"芯片","QMC6310U","LGA-8_1.2*1.2-E0.4","U2",1,150,150,2.5,{"$f":"H6*I6","v":375}]
[{"$nulls":9},{"$f":"SUM(J3:J6)","v":1855}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}