{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["R和L BOM清单-10Kpcs","前脚 BOM清单-20Kpcs","后脚 BOM清单-20Kpcs","加工"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"R和L BOM清单-10Kpcs","index":0,"n_rows":39,"n_cols":11,"rows_kept":39,"cut":false,"hidden":false,"merged":[[0,0,0,8]]}
["R和L BOM清单"]
["序号","名称","型号","封装","位号","用量","总用量","采购数量","单价","总金额","备注"]
[1,"贴片电容","0.1uF","0402C","C1, C7, C9, C14, C15, C17",6,{"$f":"F3*20000","v":120000},null,null,null,"50V"]
[2,"贴片电容","10uF","0402C","C2",1,{"$f":"F4*20000","v":20000},null,null,null,"10V"]
[3,"贴片电容","22uF","0805C","C3, C5, C16, C19",4,80000,null,null,null,"25V"]
[4,"贴片电容","1uF","0402C","C4, C18",2,40000,null,null,null,"25V"]
[5,"贴片电容","2.2uF","0402C","C6",1,20000,null,null,null,"25V"]
[6,"贴片电容","12pF","0402C","C8, C10",2,40000,null,null,null,"50V"]
[7,"贴片电容","100pF","0402C","C11",1,20000,null,null,null,"50V"]
[8,"贴片电容","1.0pF","0402C","C13",1,20000,null,null,null,"50V"]
[9,"贴片电容","10uF","0805C","C24",1,20000,null,null,null,"25V"]
[10,"贴片二极管","SS14","SOD-323","D1, D3",2,40000]
[11,"贴片LED灯","红光LED","0402LED","D2",1,20000]
[12,"贴片连接器","SH连接器，5P，1.0mm间距，卧式","SH1.0-5AW","J2",1,20000,null,null,null,"编带"]
[13,"贴片电感","3.3nH","0402L","L3",1,20000]
[14,"贴片三极管","AO3401","SOT-23-3","Q1",1,20000]
[15,"贴片三极管","AO3400","SOT-23","Q2",1,20000]
[16,"贴片电阻","3K/1%","0603RM","R1",1,20000]
[17,"贴片电阻","200K/1%","0402R","R2",1,20000]
[18,"贴片电阻","300K/1%","0402R","R3",1,20000]
[19,"贴片电阻","100K","0402R","R4, R5",2,40000]
[20,"贴片电阻","0R","0402R","R6, R9",2,40000]
[21,"贴片电阻","1K","0402R","R7, R10, R11, R12",3,60000,null,null,null,"L比R少一个R7"]
[22,"贴片电阻","4.7K","0402R","R8",1,20000]
[23,"贴片电阻","10R","0603R","R13",1,20000]
[24,"贴片电阻","10K","0402R","R14",1,20000]
[25,"芯片","TP4056X","SOP-8P","U1",1,20000]
[26,"芯片","NRF52832-QFAA-R","QFN48P-6X6","U3",1,20000]
[27,"芯片","XC6206P302MR","SOT-23","U4",1,20000,null,null,null,"TOREX/特瑞仕"]
[28,"芯片","MT9700","SOT-23-5","U7",1,20000]
[29,"晶振","32MHz/12pF/10PPM","XTAL-SMD-2016","Y1",1,20000]
[30,"PCB板",null,null,null,1,20000]
[31,"蓝牙天线","2.4G，FPC柔性25*9，3dB，线长20cm，焊接",null,null,1,20000]
[32,"4芯连接线","定制，外径1.2mm，长10cm",null,null,1,20000]
[33,"6芯连接线","定制，外径1.3mm，长10cm",null,null,1,20000]
[34,"振动电机","扁平振动电机0827，出线3cm",null,null,1,20000,null,null,null,"需要提前密封处理"]
[35,"高温电池","聚合物锂电池602530，容量>400mah",null,null,1,20000]
[36,"外壳","定制，40*27*10mm",null,null,1,20000]
[37,"磁吸充电头","定制，出线长度 ? Cm",null,null,1,20000]

{"sheet":"前脚 BOM清单-20Kpcs","index":1,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,7]]}
["前脚 BOM"]
["序号","名称","型号","封装","位号","用量","总用量","采购数量","单价","总金额"]
[1,"贴片电容","1uF","0402C","C1, C2, C3, C4",4,{"$f":"F3*20000","v":80000}]
[2,"贴片电容","10uF","0603C","C5",1,{"$f":"F4*20000","v":20000}]
[3,"芯片","LSM6DS3TR-C","LGA-14_2.5*3-e0.5","U1",1,20000]
[4,"芯片","QMC6310U","LGA-8_1.2*1.2-E0.4","U2",1,20000]
[5,"PCB板",null,null,null,1,20000]
[6,"磁铁","直径1cm，厚度1mm，钕铁硼磁",null,null,2,40000]
[7,"铁片","直径2cm，厚度 ? Mm",null,null,2,40000]
[8,"外壳","定制",null,null,1,20000]

{"sheet":"后脚 BOM清单-20Kpcs","index":2,"n_rows":9,"n_cols":10,"rows_kept":9,"cut":false,"hidden":false,"merged":[[0,0,0,7]]}
["后脚 BOM"]
["序号","名称","型号","封装","位号","用量","总用量","采购数量","单价","总金额"]
[1,"贴片电容","1uF","0402C","C3, C4",2,{"$f":"F3*20000","v":40000}]
[2,"贴片电容","10uF","0603C","C5",1,{"$f":"F4*20000","v":20000}]
[3,"芯片","QMC6310U","LGA-8_1.2*1.2-E0.4","U2",1,20000]
[5,"PCB板",null,null,null,1,20000]
[6,"磁铁","直径1cm，厚度1mm，钕铁硼磁",null,null,2,40000]
[7,"铁片","直径2cm，厚度 ? Mm",null,null,2,40000]
[8,"外壳","定制",null,null,1,20000]

{"sheet":"加工","index":3,"n_rows":5,"n_cols":10,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,9]]}
["加工"]
["序号","名称","型号","封装","位号","用量","总用量","采购数量","单价","总金额"]
[1,"SMT加工","包括钢网"]
[2,"手工焊接"]
[3,"灌胶"]